Tinnies 1, 2 and 4 are BMRC tinnies.

Tinny 3 is not to be used for coaching as it belongs to Rowing ACT.

**The maximum load for each tinny is 3 people (total weight 270K)**

**It is the responsibility of the tinny operator to check the following:**

|  |
| --- |
| **LICENCING/BOAT PERMIT** |
| CARRY YOUR TINNY LICENCE WHILE OPERATING THE TINNY (Power boat licence or TL3 certificate) |
| CURRENT VESSEL PERMIT ATTACHED TO THE SIDE OF THE TINNY |
| **MAINTENANCE** |
| SUFFICIENT/CORRECT FUEL |
| NO DAMAGE/LEAKS EVIDENT |
| BUNG PRESENT/FITTED PROPERLY |
| **SAFETY EQUIPMENT** |
| PADDLE X1 |
| BAILING BUCKET X1 |
| ANCHOR/ROPE/CHAIN X1 |
| ELECTRIC TORCH X1 (IN WORKING ORDER) |
| SAFETY LIGHT/LIGHTED LANTERN (MUST BE FITTED BEFORE SUNRISE AND AFTER SUNSET) |
| SUFFICIENT PFDs FOR THE NUMBER OF OCCUPANTS |
| FIRE EXTINGUISHER (SERVICING DATE CURRENT) |
| **EMERGENCY EQUIPMENT**: |
| MOBILE PHONE OR TWO WAY RADIO |
| EMERGENCY CONTACTS/LOCATION OF EMERGENCY TELEPHONES AROUND THE LAKE |
| FIRST AID KIT |
| SPARE LIGHTS (FOR TINNY AND ROWING BOATS) |
| THERMAL (SPACER) BLANKET (X2) |
| THROW LINE |
| COMPASS AND MAP (IN CASE OF FOG) |

**Report maintenance issues to the Vice-Captain directly if urgent , or via the maintenance log.**

**Report safety/emergency equipment issues to the Captain, Vice-Captain, Safety Officer**